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	Key Features:
· GENSTAR IVS 2.0 - AI Analytics (Artificial Intelligence) - artificial intelligence using DeepLearning algorithms for instant and precise detection and recognition of objects such as persons and vehicles.
· Smart Encode - dynamically adapts network stream and codec parameters to maintain recording continuity while minimizing archive storage requirements.
· Image sensor schedules - image sensor operation can be configured based on time or Day/Night mode.
· Corridor mode - adapts the field of view to scenes with a significant disproportion between the height and width of the monitored area.
· Supports detection of faces/persons/vehicles
· Supports P2P cloud
· NDAA compliant - device compliant with the U.S. National Defense Authorization Act.

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	IP camera with GENSTAR IVS 2.0 analytics
	[image: Obraz zawierający Czcionka, Grafika, projekt graficzny, zrzut ekranu

Opis wygenerowany automatycznie]    
	
	

	
	
	

	Model
	ZN8-53B5M213T-J1
	
	

	Image sensor
	1/3" progressive scan CMOS
	
	

	Sensitivity (AGC ON)
	Color: 0.01 lux @ F1.6 / IR ON: 0 lux
	
	

	Day/Night mode
	Automatic IR-cut filter
	
	

	Electronic shutter
	1/5 - 1/20,000
	
	

	Iris
	Fixed Iris
	
	

	WDR mode
	d-WDR
	
	

	Noise reduction
	2D  /  3D-DNR
	
	

	Lens
	Motorized zoom with AF: 2.7 - 13.5 mm, H: 90° - 29.8°
	
	

	IR illuminator
	4 x IR LED, range up to 60 m, 850 nm
	
	

	AV compression
	H.265 | H.264 | MJPEG | G.711U | G.711A | RAW
	
	

	Bitrate (CBR/VBR)

	Stream 1: 200 Kbps - 12 Mbps
	
	

	
	Streams 2/3: 100 Kbps - 6/3 Mbps
	
	

	Resolution 
and frame rate
	2560×1920, 2560x1440, 2304x1296 (25 fps)
	
	

	
	1920x1080 and 1280x720 (25 fps)
	
	AI analytics capabilities: GENSTAR IVS 2.0

	Video streams
	Stream 1: max. 2560x1920 (5MP)
	
	AI engine features
(Artificial Intelligence)
	Object detection: DeepLearning engine

	
	Stream 2: D1, VGA, CIF
	
	
	Detection: face, person, vehicle.

	
	Stream 3: VGA, CIF, QVGA
	
	
	Object classification: person, vehicle (Detector)

	Image settings
	Rotation, saturation, brightness, contrast, sharpness
	
	
	Simultaneous multi-object tracking (Tracker)

	Digital functions
	HLC | BLC | ROI | DEFOG
	
	Behavioral detection
	Intrusion, loitering, wrong direction, illegal parking, people counting,

	Corridor mode
	Yes (9:16)
	
	
	Single/double perimeter line crossing.

	Privacy masks
	4 zones
	
	
	

	Events
	Motion detection (22x18 grid),
	
	
	

	
	GENSTAR IVS 2.0 analytics, D/N switching,
	
	Technical Specifications

	Network protocols
	IPv4/IPv6, HTTP/HTTPS, DNS, DDNS, DHCP,
	
	Reset button
	Yes

	
	PPPoE, RTSP/ RTCP/RTP, TCP/UDP, NTP, ARP
	
	SD card support
	MicroSD card slot, max. 1 TB

	
	UPnP, FTP, SMTP, QoS, ICMP, IGMP, SMTP
	
	Power supply
	12VDC  /  PoE  (802.3af / class-3)

	
	802.1x, SNMP, Multicast
	
	Microphone
	Yes, built-in

	RTSP support
	Standard RFC2326 (VLC Player / QuickTime)
	
	Power consumption
	1.6 W (IR-LED OFF)  /  5W (IR-LED ON)

	Security
	User authentication, hardware WatchDog
	
	Power output
	N/D

	Compatibility
	ONVIF (Profile S/T/G/M), SDK, CGI
	
	Operating temperature
	-30°C … +50°C

	Ethernet interface
	10/100 Base-T, RJ45
	
	Max. humidity
	90%

	Audio
	N/D
	
	Certifications
	CE  /  FCC  /  IP66 

	Alarm
	N/D
	
	Dimensions / weight
	Ø 130 mm (base) x 113 mm / 720 g

	Analog output
	N/D
	
	Adjustment range
	355° (H) / 75° (V) / 355° (sensor rotation)


			Security

	OS / Firmware protection
	Encrypted firmware, secure boot, signed firmware

	User authentication
	Digest authentication, brute-force attack protection

	Network authentication
	IEEE 802.1X (EAP-TLS)

	Secure communication
	HTTPS, WSS (WebSocket Secure), SRTP

	Access control
	IP-based access control, automatic logout

	Data protection
	Credential encryption

	Secure data storage
	SD card partition encryption using AES-256 and hardware Secure Element

	Audit
	Access / system / event log management

	Supply chain security
	SBOM





Built-in GSTAR IVS 2.0 video analytics (AI Analytics)
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Zawartość wygenerowana przez AI może być niepoprawna.]
AI multi-object
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Intrusion
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Smart detection
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   Line crossing
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Double line
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                   Group loitering
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Wrong direction
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Illegal parking
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                   People counting





	DORI Distance

	[bookmark: _Hlk189821489]Lens
	Detection
	Observation
	Recognition
	Identification

	2.8mm
	82 m
	32.8 m
	16.4 m
	7.2 m

	OODPCVS Distance (OODPCVS distances calculated based on pixel density thresholds according to IEC/EN 62676-4:2025.)

	General overview
	Object outline
		



	Object discrimination



	Behavior perception
	Object characterization
	Verification
	Detailed analysis

	117.5 – 342.5 m
	58.8 – 171.3 m
	29.4 – 85.6 m
	18.8 – 54.8 m
	9.4 – 27.4 m
	4.7 – 13.7 m
	1.6 – 4.6 m





	

	Mounting 
adapters:
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	ZA8-CBK627B only in combination with ZA8-JBMP-2


	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	ZA8-CBK656A
	ZA8-CBK627B
	
	
	
	
	

	
	 

	
	
	
	
	
	

	
	
	
	
	
	
	
	

	Compatibility:
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	GENSTAR NVR
	CORTROL VMS
	NDAA Compliance
	
	
	








	
	
	

	Dimensions:
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